===========================
== Updater user guide
== Ver 1.0.0
== 2008.12.08
===========================

1.  Prepare the environment 
===========================
	a. Prepare a PC with Windows XP OS.
	a. Prepare the latest usb driver and updater software.
	b. Connect the USB update cable from the PC to the monitor's GPI port.
	c. Connect power cable to the monitor.

2.  Put the monitor into update mode
===========================
	a. Hit the following keys in the key board of monitor in order.
	"MENU", "ENTER", "UP", "DOWN","MENU", "ENTER", "UP", "DOWN", "MENU", "UP"
	b. Hit the "POWER" key

3. Install the usb driver
===========================
	If this is the first time for the PC to update firmware, 
		windows will prompt a new device found. Follow the wizard to install 
		the usb driver.

4. Update the Firmware  
==========================
	a. Launch the "Usbupdater" software.
	b. Press the "Select Image" button to select a proper firmware img file.
	c. Check the Mode and version.
	d. Press the "Update" button
	e. Wait until the update progress bar finishes and pop up a "Succeeded updating the firmware." dialog. 
		This will take about two minutes. 


Errors and resolustion
======================
Sometimes "Usbupdater" will popup a dialog for some errors.

	"This file is corrupted or not an image file!"	- The firmware img file is corrupted or not a img file

	"Version misMatch."	- img file version mismatch with the "Usbupdater" software, make sure the "Usbupdater"
				  software is the latest.

	"Can't open target."
	"Can't connect target."
	"No target found."	- Make sure the monitor is power on and the usb driver installed proper
				  If those are all ok maybe the monitor does not enter "update mode", power off the monitor and
				  goto step 2 again.